|  |  |
| --- | --- |
| mtd issue form |  |
| Targets /Simulators |  |  |  | **Maintenance will be available from 0700 – 1600 M-F:** **760-725-4805 / 760-399-6369** |
| Requested by phone (Rank, Full Name) | DOD ID # | Unit | Phone # /Cell | Issue Date | Return Date |
|  |  |  |  | Click here to enter a date. | Click here to enter a date. |
| Issued to (If not same as above) | Email address | Company/S-3 # (Must be different from above number) |
|  |  |  |  |
|  |
| Qty | Type of Targets and Accessories | Customer Initials | ESP Tech Initials on Return / Notes |
|  | Choose an item. |  |  |
|  | Choose an item. |  |  |
|  | Choose an item. |  |  |
|  | Choose an item. |  |  |
|  | Choose an item. |  |  |
|  | Choose an item. |  |  |
|  | Choose an item. |  |  |
|  | Choose an item. |  |  |
|  | Choose an item. |  |  |
|  | Choose an item. |  |  |
|  | Choose an item. |  |  |
|  | Other: |  |  |
|  |  |  |  |

**PITS classes consists of:**

* The proper items needed to operate a target.
* How to properly place target w/shield.
* How to properly connect the battery.
* How to operate the remote.
* How to transport and load the systems.
* Different types of trouble shooting.
* How to properly recharge batteries.

**Simulator classes consist of:**

* The proper items needed to operate the simulator.
* How to properly setup simulator (pressures/cables).
* How to properly connect the battery.
* How to operate the remote.
* How to transport and load the systems
* Different types of trouble shooting
* How to properly recharge batteries.

You have gotten training on this today or before and feel comfortable with the system initial here:

 \_\_\_\_\_\_\_\_\_\_

**a. General info: All training devices must be cleaned of excessive mud/dirt or debris prior to return Do not lose, break, misuse or otherwise damage training systems. Ensure that all accessories (SL3 items) are inventoried and complete upon turn in.**

**b. PITS: Units must provide 10-12 filled sand bags per target. THE SHIELD MUST NOT BE SEEN WHEN COVERED WITH SANDBAGS. One steel shield per target is required and is provided by TSD. Place the battery behind the shield to prevent damage. PITS may only be engaged by 5.56mm, 7.62mm and 50 caliber, direct fire. Minimum standoff for engagement: 5.56mm is 25 meters, 7.62mm and .50 cal is 100 meters.**

**c. All items must be returned on or before the specified return date. Please notify us immediately if you are unable to return as specified. Send all correspondence to: MCB\_CamPen\_TSD\_Trg\_Dev@NMCI.USMC.Mil 760-725-6139**

**d. LARUE TARGETS: Larue reactive steel targets require 2 sandbags per to cover the top and the side of the lifter mechanism. The .50 cal model will be issued with its own shield. Larue static targets (LTCB) “chain bangers” require sandbags in the amount sufficient to cover the stand to protect it from damage. Additionally, if you paint the target silhouettes any color other than black, you must re-paint them black before returning the targets. Standard Larue targets may only be engaged by 5.56mm and 7.62mm, direct fire. The .50 cal model may be engaged by 5.56mm, 7.62mm and .50 cal. Larue minimum standoff for engagement: 5.56mm, 7.62mm, .50 cal is 100 meters.**